{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":26,"n_cols":6,"rows_kept":26,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FFA-A9 / RXM-A"]
[]
[]
[]
[]
["","","","","FFA50A2VEB9 / RXM50A5V1B","FFA60A2VEB9 / RXM60A5V1B"]
["Učin hlađenja","Nom.","","kW","5.00","5.7"]
["Učin grijanja","Nom.","","kW","5.80","7"]
["Nazivna učinkovitost","EER","","","3.24","3.05"]
["","COP","","","3.49","3.41"]
["","Godišnja potrošnja energije","","kWh","772","931"]
["","Direktiva o označivanju energetske učinkovitosti","Hlađenje","","A","B"]
["","","Grijanje","","B","B"]
["Hlađenje prostora","Razred energetske učinkovitosti","","","A+","A+"]
["","Kapacitet","Pdesign","kW","5.00","5.7"]
["","SEER","","","5.98","5.76"]
["","Godišnja potrošnja energije","","kWh/a","293","346"]
["Grijanje prostora (prosječna klima)","Razred energetske učinkovitosti","","","A","A+"]
["","Kapacitet","Pdesign","kW","3.84","3.96"]
["","SCOP/A","","","3.90","4.04"]
["","Pdh kapacitet grijanja pri -10°","","kW","3.40","3.5"]
["","Godišnja potrošnja energije","","kWh/a","1378","1373"]
["Napomene","","","","","(1) - Nom. kapacitet hlađenja se temelji se na sljedećim parametrima: unutarnja temperatura: 27 °C DB, 19 °C WB, vanjska temperatura: 35 °C DB, odgovarajuće cijevi rashladnog sredstva: 5 m, razlika u visini: 0m."]
["","","","","","(2) - Nazivni učin grijanja zasnovani su na: unutarnja temperatura: 20°C DB, vanjska temperatura : 7°C DB, 6°C WB, odgovarajući cjevovod za radnu tvar: 5 m, razlika razine: 0 m."]
["","","","","","(3) - Pogledajte odvojene nacrte za radno područje"]
["","","","","","(4) - Vidi električne podatke na posebnim nacrtima"]