{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":27,"n_cols":5,"rows_kept":27,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FLXS-B9 / RXS-L"]
[]
[]
[]
[]
["","","","","FLXS35BAVMB9 / RXS35L2V1B"]
["Učin hlađenja","Min.","","kW","1.2"]
["","Maks.","","kW","3.8"]
["","Nom.","","kW","3.5"]
["Priključci cjevovoda","Tekućina","VP","mm","6.35"]
["","Plin","VP","mm","9.5"]
["","Odvod vode","OD","mm","18.0"]
["Nazivna učinkovitost","Godišnja potrošnja energije","","kWh","565"]
["","EER","","","3.10"]
["","COP","","","3.57"]
["","Direktiva o označivanju energetske učinkovitosti","Hlađenje","","B"]
["","","Grijanje","","B"]
["Kapacitet grijanja","Nom.","","kW","4.0"]
["","Min.","","kW","1.4"]
["","Maks.","","kW","5.0"]
["Napomene","","","","(1) - EER/COP prema Eurovent 2012, za korištenje samo izvan EU"]
["","","","","(2) - 220 V"]
["","","","","(3) - 230 V"]
["","","","","(4) - 240 V"]
["","","","","(5) - Hlađenje: unutarnja temperatura 27°CDB, 19,0°CWB; vanjska temperatura 35°CDB; 24°CWB, duljina odgovarajućeg cjevovoda: 5 m"]
["","","","","(6) - Grijanje: unutarnja temperatura 20°CDB, vanjska temperatura 7°CDB, 6°CWB, odgovarajući cjevovod za radnu tvar: 5 m"]
["","","","","(7) - Nazivna učinkovitost: hlađenje na 35°/27° nazivnog opterećenja, grijanje na 7°/20° nazivnog opterećenja"]