{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":44,"n_cols":5,"rows_kept":44,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FLXS-B9"]
[]
[]
[]
[]
["","","","","FLXS35BAVMB9"]
["Razina tlaka zvuka","Grijanje","Visoko","dBA","46"]
["","","Tihi način rada","dBA","30"]
["","","Nizak","dBA","33"]
["","Hlađenje","Tihi način rada","dBA","29"]
["","","Nizak","dBA","32"]
["","","Visoko","dBA","38"]
["","","Nom.","dBA","36"]
["","Hlađenje","Nom.","dBA","35"]
["Standardna dodatna oprema","Priručnik za instalaciju","","","1"]
["","Radni priručnik","","","1"]
["","Infracrveno daljinsko upravljanje","","","1"]
["","AAA suhe baterije","","","2"]
["","Držač daljinskog upravljača","","","1"]
["","Montažna ploča","","","1"]
["","Cijev za izolaciju topline (cijev za rashladnu tekućinu)","","","8"]
["","Filtar za pročišćavanje zraka","","","1"]
["","Fotokatalitički deodorizirajući filtar","","","1"]
["","Bočni pokrov","","","2"]
["","Povezna traka","","","4"]
["Upravljački sustavi","Infrared remote control","","","ARC433B67"]
["Promjer cjevovoda","Liquid","OD","mm","6.35"]
["","Plin","OD","mm","9.5"]
["","Odvod vode","","","18"]
["Sound power level","Hlađenje","","dBA","53"]
["","Grijanje","","dBA","59"]
["Dimenzije","Jedinica","Širina","mm","1,050"]
["","","Dubina","mm","200"]
["","","Visina","mm","490"]
["Kućište","Colour","","","Badem bijela"]
["Težina","Jedinica","","kg","16"]
["Power supply","Phase","","","1~"]
["","Frekvencija","","Hz","50"]
["","Naziv","","","VM"]
["","Napon","","V","220-240"]
["Napomene","","","","(1) - 220 V"]
["","","","","(2) - 230 V"]
["","","","","(3) - 240 V"]
["","","","","(4) - Kada se spaja s vanjskom jedinicom za više sustava, pogledajte tehničke podatke vanjske jedinice za više sustava koju treba spojiti."]