{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":37,"n_cols":10,"rows_kept":37,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXA-BT / RXA-A"]
[]
[]
[]
[]
["","","","","FTXA20B2V1BT / RXA20A5V1B","FTXA20B2V1BT / RXA20A3V1B","FTXA25B2V1BT / RXA25A3V1B","FTXA25B2V1BT / RXA25A5V1B","FTXA35B2V1BT / RXA35A5V1B","FTXA35B2V1BT / RXA35A3V1B"]
["Učin hlađenja","Min.","","kW","1.3","1.3","1.3","","1.4","1.4"]
["","Maks.","","kW","2.6","2.6","3.2","","4.0","4.0"]
["","Nom.","","kW","2.0","2.0","2.5","","3.4","3.4"]
["Nazivna učinkovitost","EER","","","4.70","4.70","4.46","","4.37","4.37"]
["","COP","","","5.00","5.00","5.00","","4.04","4.04"]
["","Direktiva o označivanju energetske učinkovitosti","Hlađenje","","A","A","A","","A","A"]
["","","Grijanje","","A","A","A","","A","A"]
["Kapacitet grijanja","Nom.","","kW","2.50","2.50","2.80","","4.00","4.00"]
["","Min.","","kW","1.30","1.30","1.30","","1.40","1.40"]
["","Maks.","","kW","3.50","3.50","4.70","","5.20","5.20"]
["Outdoor unit","","","","","RXA20A2V1B","RXA25A2V1B","RXA25A5V1B","","RXA35A2V1B"]
["Učin hlađenja","Min.","","kW","","","","1.3"]
["","Nom.","","kW","","","","2.5"]
["","Maks.","","kW","","","","3.2"]
["Učin grijanja","Min.","","kW","","","","1.30"]
["","Nom.","","kW","","","","2.80"]
["","Maks.","","kW","","","","4.70"]
["Nazivna učinkovitost","EER","","","","","","4.46"]
["","COP","","","","","","5.00"]
["","Direktiva o označivanju energetske učinkovitosti","Hlađenje","","","","","A"]
["","","Grijanje","","","","","A"]
["Hlađenje prostora","Razred energetske učinkovitosti","","","","","","A+++"]
["","Kapacitet","Pdesign","kW","","","","2.50"]
["","SEER","","","","","","8.74"]
["","Godišnja potrošnja energije","","kWh/a","","","","101"]
["Grijanje prostora (prosječna klima)","Razred energetske učinkovitosti","","","","","","A+++"]
["","Kapacitet","Pdesign","kW","","","","2.45"]
["","SCOP/A","","","","","","5.15"]
["","Pdh kapacitet grijanja pri -10°","","kW","","","","2.30"]
["","Godišnja potrošnja energije","","kWh/a","","","","666"]
["Raspon energetske učinkovitosti","","","","","","","A+++ ~ D"]