{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":50,"n_cols":9,"rows_kept":50,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXA-CS"]
[]
[]
[]
[]
["","","","","","FTXA20C2V1BS","FTXA25C2V1BS","FTXA42C2V1BS","FTXA50C2V1BS"]
["Ulazna struja","Hlađenje","","Nom.","kW","0.02","0.022","0.028","0.030"]
["","Grijanje","","Nom.","kW","0.02","0.02","0.036","0.039"]
["Kućište","Boja","","","","Srebrni","Srebrni","Srebrni","Srebrni"]
["Dimenzije","Uređaj","","Visina","mm","295","295","295","295"]
["","","","Širina","mm","798","798","798","798"]
["","","","Dubina","mm","189","189","189","189"]
["Težina","Uređaj","","","kg","11.5","11.5","11.5","11.5"]
["Ventilator","Količina zraka","Hlađenje","Visoko","m³/min","11","11.5","13.1","13.5"]
["","Protok zraka","Hlađenje","Srednji","m³/min","8.2","8.6","9.8","10.4"]
["","","","Nizak","m³/min","6.1","6.1","7.2","7.6"]
["","","","Tihi način rada","m³/min","4.6","4.6","4.6","5.2"]
["","","Grijanje","Visoko","m³/min","10.9","11.1","14.6","15.1"]
["","Protok zraka","Grijanje","Srednji","m³/min","8.7","9","10.5","11.1"]
["","","Grijanje","Nizak","m³/min","6.4","6.4","7.7","8.2"]
["","","","Tihi način rada","m³/min","4.5","4.5","5.2","5.7"]
["Zvučna snaga","Hlađenje","","","dBA","57","57","60","60"]
["Razina tlaka zvuka","Hlađenje","","Visoko","dBA","39","40","45","46"]
["Razina zvučnog tlaka","Hlađenje","","Srednji","dBA","32","33","37","39"]
["Razina tlaka zvuka","Hlađenje","","Nizak","dBA","25","25","29","31"]
["","","","Tihi način rada","dBA","19","19","21","24"]
["","Grijanje","","Visoko","dBA","39","40","45","46"]
["Razina zvučnog tlaka","Grijanje","","Srednji","dBA","32","33","37","42"]
["Razina tlaka zvuka","Grijanje","","Nizak","dBA","25","25","29","33"]
["","","","Tihi način rada","dBA","19","19","21","24"]
["Radna tvar","GWP","","","","675","675","675","675.0"]
["Priključci cjevovoda","Tekućina","","VP","mm","6.35","6.35","6.35","6.35"]
["","Plin","","VP","mm","9.5","9.5","9.5","12.70"]
["","Odvod vode","","","","18","18","18","18"]
["Upravljački sustavi","Infracrveno daljinsko upravljanje","","","","ARC466A85","ARC466A85","ARC466A85","ARC466A85"]
["","Žično daljinsko upravljanje","","","","BRC073A1","BRC073A1","BRC073A1","BRC073A1"]
["Standardna dodatna oprema","Installation manual","","","","1","1","1","1"]
["","Screw cover","","","","2","2","2","2"]
["","AAA dry-cell batteries","","","","2","2","2","2"]
["","General safety precautions","","","","1","1","1","1"]
["","Operation manual","","","","1","1","1","1"]
["","Zračni filtar","","","","2","2","2","2"]
["","Infrared remote control","","","","1","1","1","1"]
["","Remote controller mounting plate","","","","1","1","1","1"]
["","Screw bag","","","","1","1","1","1"]
["Napajanje","Naziv","","","","V1","V1","V1","V1"]
["","Faza","","","","1~","1~","1~","1~"]
["","Frekvencija","","","Hz","50","50","50","50"]
["","Napon","","","V","220-240","220-240","220-240","220-240"]
["Raspon energetske učinkovitosti","","","","","","","","A+++ ~ D"]