{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":38,"n_cols":6,"rows_kept":38,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXF-B"]
[]
[]
[]
[]
["","","","","FTXF20B5V1B","FTXF25B5V1B"]
["Razina tlaka zvuka","Grijanje","Visoko","dBA","39","40"]
["","","Srednji","dBA","34","34"]
["","","Tihi način rada","dBA","21","21"]
["","","Nizak","dBA","28","28"]
["","Hlađenje","Srednji","dBA","33","33"]
["","","Tihi način rada","dBA","20","20"]
["","","Nizak","dBA","25","26"]
["","","Visoko","dBA","39","40"]
["Standardna dodatna oprema","Priručnik za instalaciju","","","1","1"]
["","Radni priručnik","","","1","1"]
["","Infracrveno daljinsko upravljanje","","","1","1"]
["","AAA suhe baterije","","","2","2"]
["","Držač daljinskog upravljača","","","1","1"]
["","Montažna ploča","","","1","1"]
["","Učvrsni vijak unutarnje jedinice","","","2","2"]
["Control systems","Wired remote control","","","BRC944B2, BRC073A1","BRC944B2, BRC073A1"]
["","Infrared remote control","","","ARC470A1","ARC470A1"]
["Priključci cjevovoda","Tekućina","VP","mm","6.35","6.35"]
["","Plin","VP","mm","9.50","9.50"]
["","Odvod vode","","","18","18"]
["Ulazna struja","Hlađenje","Nom.","kW","0.017","0.019"]
["","Grijanje","Nom.","kW","0.020","0.020"]
["Sound power level","Hlađenje","","dBA","55","55"]
["","Grijanje","","dBA","55","55"]
["Dimenzije","Unit","Width","mm","770","770"]
["","","Depth","mm","225","225"]
["","","Height","mm","286","286"]
["Kućište","Boja","","","Bijelo","Bijelo"]
["Težina","Jedinica","","kg","8.50","8.50"]
["Power supply","Faza","","","1~","1~"]
["","Frekvencija","","Hz","50","50"]
["","Napon","","V","220-240","220-240"]