{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":30,"n_cols":9,"rows_kept":30,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXF-F / RXF-F"]
[]
[]
[]
[]
["","","","","FTXF20F5V1B / RXF20F5V1B","FTXF25F5V1B / RXF25F5V1B","FTXF35F5V1B / RXF35F5V1B","FTXF42F5V1B / RXF42F5V1B","FTXF50F5V1B / RXF50F5V1B"]
["Vanjska jedinica","","","","RXF20F5V1B","RXF25F5V1B","RXF35F5V1B","RXF42F5V1B","RXF50F5V1B"]
["Učin hlađenja","Min.","","kW","1.3","1.30","1.30","1.4","1.30"]
["","Nom.","","kW","2","2.50","3.30","4.2","5"]
["","Maks.","","kW","2.4","2.80","3.80","4.3","5.30"]
["Učin grijanja","Min.","","kW","1.3","1.30","1.30","1.4","1.43"]
["","Nom.","","kW","2.4","2.80","3.50","4.6","5.40"]
["","Maks.","","kW","3.3","3.70","4.40","5","6.13"]
["Nazivna učinkovitost","EER","","","3.38","3.24","3.30","3.3","3.30"]
["","COP","","","3.75","3.73","3.72","3.71","3.71"]
["","Godišnja potrošnja energije","","kWh","108","135","188","226","269"]
["","Direktiva o označivanju energetske učinkovitosti","Hlađenje","","A","A","A","A","A"]
["","","Grijanje","","A","A","A","A","A"]
["Hlađenje prostora","Razred energetske učinkovitosti","","","A++","A++","A++","A++","A++"]
["","Kapacitet","Pdesign","kW","2","2.50","3.50","4.2","5"]
["","SEER","","","6.5","6.50","6.50","6.5","6.50"]
["","Godišnja potrošnja energije","","kWh/a","108","135","188","226","269"]
["Grijanje prostora (prosječna klima)","Razred energetske učinkovitosti","","","A+","A+","A+","A+","A+"]
["","Kapacitet","Pdesign","kW","2.2","2.40","2.60","3.3","3.80"]
["","SCOP/A","","","4.2","4.20","4.20","4.3","4.10"]
["","Pdh kapacitet grijanja pri -10°","","kW","1.86","1.97","2.21","2.61","3.24"]
["","Godišnja potrošnja energije","","kWh/a","733","801","867","1,075","1,297"]
["Napomene","","","","(1) - Nazivni učini hlađenja se temelje na: unutarnjoj temperaturi: 27 °CDB, 19 °CWB, vanjskoj temperaturi: 35 °CDB, ekvivalentnom cjevovodu radne tvari: 5 m, razlici u visini: 0 m. Podaci za seriju visoke učinkovitosti, certifikat Eurovent","(1) - Nazivni učini hlađenja se temelje na: unutarnjoj temperaturi: 27 °CDB, 19 °CWB, vanjskoj temperaturi: 35 °CDB, ekvivalentnom cjevovodu radne tvari: 5 m, razlici u visini: 0 m. Podaci za seriju visoke učinkovitosti, certifikat Eurovent","(1) - Nazivni učini hlađenja se temelje na: unutarnjoj temperaturi: 27 °CDB, 19 °CWB, vanjskoj temperaturi: 35 °CDB, ekvivalentnom cjevovodu radne tvari: 5 m, razlici u visini: 0 m. Podaci za seriju visoke učinkovitosti, certifikat Eurovent","(1) - Nazivni učini hlađenja se temelje na: unutarnjoj temperaturi: 27 °CDB, 19 °CWB, vanjskoj temperaturi: 35 °CDB, ekvivalentnom cjevovodu radne tvari: 5 m, razlici u visini: 0 m. Podaci za seriju visoke učinkovitosti, certifikat Eurovent","(1) - Nazivni učini hlađenja se temelje na: unutarnjoj temperaturi: 27 °CDB, 19 °CWB, vanjskoj temperaturi: 35 °CDB, ekvivalentnom cjevovodu radne tvari: 5 m, razlici u visini: 0 m. Podaci za seriju visoke učinkovitosti, certifikat Eurovent"]
["","","","","(2) - Nazivni učini grijanja temelje se na: unutarnjoj temperaturi: 20 °CDB, vanjskoj temperaturi: 7 °CDB, 6 °CWB, ekvivalentnom cjevovodu radne tvari: 5 m, razlici u visini: 0 m. Podaci za seriju standardne učinkovitosti","(2) - Nazivni učini grijanja temelje se na: unutarnjoj temperaturi: 20 °CDB, vanjskoj temperaturi: 7 °CDB, 6 °CWB, ekvivalentnom cjevovodu radne tvari: 5 m, razlici u visini: 0 m. Podaci za seriju standardne učinkovitosti","(2) - Nazivni učini grijanja temelje se na: unutarnjoj temperaturi: 20 °CDB, vanjskoj temperaturi: 7 °CDB, 6 °CWB, ekvivalentnom cjevovodu radne tvari: 5 m, razlici u visini: 0 m. Podaci za seriju standardne učinkovitosti","(2) - Nazivni učini grijanja temelje se na: unutarnjoj temperaturi: 20 °CDB, vanjskoj temperaturi: 7 °CDB, 6 °CWB, ekvivalentnom cjevovodu radne tvari: 5 m, razlici u visini: 0 m. Podaci za seriju standardne učinkovitosti","(2) - Nazivni učini grijanja temelje se na: unutarnjoj temperaturi: 20 °CDB, vanjskoj temperaturi: 7 °CDB, 6 °CWB, ekvivalentnom cjevovodu radne tvari: 5 m, razlici u visini: 0 m. Podaci za seriju standardne učinkovitosti"]
["","","","","(3) - Vidi električne podatke na posebnim nacrtima","(3) - Vidi električne podatke na posebnim nacrtima","(3) - Vidi električne podatke na posebnim nacrtima","(3) - Vidi električne podatke na posebnim nacrtima","(3) - Vidi električne podatke na posebnim nacrtima"]