{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":51,"n_cols":12,"rows_kept":51,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXF-F"]
[]
[]
[]
[]
["","","","","","FTXF20F5V1B","FTXF25F5V1B (Archived)","FTXF35F5V1B (Archived)","FTXF42F5V1B (Archived)","FTXF50F5V1B (Archived)","FTXF60F2V1B (Archived)","FTXF71F2V1B (Archived)"]
["Ulazna struja","Hlađenje","","Nom.","kW","0.023","0.023","0.029","0.04","0.04","0.032","0.032"]
["","Grijanje","","Nom.","kW","0.023","0.023","0.029","0.04","0.04","0.035","0.035"]
["Kućište","Boja","","","","Bijelo","Bijelo","Bijelo","Bijelo","Bijelo","Bijelo","Bijelo"]
["Dimenzije","Uređaj","","Visina","mm","286","286","286","286","286","295","295"]
["","","","Širina","mm","770","770","770","770","770","990","990"]
["","","","Dubina","mm","225","225","225","225","225","263","263"]
["Težina","Uređaj","","","kg","8","8","8.5","9","9","13.5","13.5"]
["Ventilator","Količina zraka","Hlađenje","Visoko","m³/min","9.8","10","11.5","12.6","12.6","17.3","17.3"]
["","Protok zraka","Hlađenje","Srednji","m³/min","8","8","8","9","9","14.8","14.8"]
["","","","Nizak","m³/min","6","6.2","6.4","6.9","7.2","12.2","12.2"]
["","","","Tihi način rada","m³/min","4.3","4.3","4.4","4.9","6.4","10.7","10.7"]
["","","Grijanje","Visoko","m³/min","10.4","10.4","11.9","12.8","12.8","17.9","17.9"]
["","Protok zraka","Grijanje","Srednji","m³/min","8.3","8.4","8.6","8.8","9.6","15.8","15.8"]
["","","Grijanje","Nizak","m³/min","6.2","6.4","6.5","6.7","7.2","12.8","12.8"]
["","","","Tihi način rada","m³/min","5.3","5.3","5.3","5.2","6.4","11.3","11.3"]
["Zvučna snaga","Hlađenje","","","dBA","53","54","54","59","59","60","62"]
["","Grijanje","","","dBA","55","55","56","59","59","62","62"]
["Razina tlaka zvuka","Hlađenje","","Visoko","dBA","39","40","43","45","45","45","46"]
["Razina zvučnog tlaka","Hlađenje","","Srednji","dBA","33","33","34","36","39","41","42"]
["Razina tlaka zvuka","Hlađenje","","Nizak","dBA","25","26","27","30","34","36","37"]
["","","","Tihi način rada","dBA","20","20","20","22","31","33","34"]
["","Grijanje","","Visoko","dBA","39","40","40","44","44","44","45"]
["Razina zvučnog tlaka","Grijanje","","Srednji","dBA","34","34","35","34","38","40","41"]
["Razina tlaka zvuka","Grijanje","","Nizak","dBA","28","28","29","28","33","35","36"]
["","","","Tihi način rada","dBA","21","21","21","22","30","32","33"]
["Priključci cjevovoda","Tekućina","","VP","mm","6","6","6","6","6","6.35","6.35"]
["","Plin","","VP","mm","9.5","9.5","9.5","9.5","12.7","12.7","12.7"]
["","Odvod vode","","","","18","18","18","18","18","18","18"]
["Upravljački sustavi","Infracrveno daljinsko upravljanje","","","","ARC480A93","ARC480A93","ARC480A93","ARC480A93","ARC480A93","ARC470A1","ARC470A1"]
["","Žično daljinsko upravljanje","","","","BRC073A1","BRC073A1","BRC073A1","BRC073A1","BRC073A1","BRC073A1","BRC073A1"]
["Standardna dodatna oprema","Installation manual","","","","1","1","1","1","1","1","1"]
["","AAA dry-cell batteries","","","","2","2","2","2","2","2","2"]
["","General safety precautions","","","","1","1","1","1","1"]
["","Operation manual","","","","1","1","1","1","1","1","1"]
["","Indoor unit fixing screws","","","","2","2","2","2","2","2","2"]
["","Infrared remote control","","","","1","1","1","1","1","1","1"]
["","Mounting plate","","","","1","1","1","1","1","1","1"]
["","Remote control holder","","","","1","1","1","1","1","1","1"]
["Napajanje","Naziv","","","","","","","","","V1","V1"]
["","Faza","","","","1~","1~","1~","1~","1~","1~","1~"]
["","Frekvencija","","","Hz","50","50","50","50","50","50","50"]
["","Napon","","","V","220-440","220-440","220-440","220-440","220-440","220-240","220-240"]
["Napomene","","","","","(1) - Hlađenje: unutarnja temperatura 27°CDB, 19°CWB; vanjska temperatura 35°CDB; duljina odgovarajućeg cjevovoda: 5 m; razlika razine: 0 m","(1) - Hlađenje: unutarnja temperatura 27°CDB, 19°CWB; vanjska temperatura 35°CDB; duljina odgovarajućeg cjevovoda: 5 m; razlika razine: 0 m","(1) - Hlađenje: unutarnja temperatura 27°CDB, 19°CWB; vanjska temperatura 35°CDB; duljina odgovarajućeg cjevovoda: 5 m; razlika razine: 0 m","(1) - Hlađenje: unutarnja temperatura 27°CDB, 19°CWB; vanjska temperatura 35°CDB; duljina odgovarajućeg cjevovoda: 5 m; razlika razine: 0 m","(1) - Hlađenje: unutarnja temperatura 27°CDB, 19°CWB; vanjska temperatura 35°CDB; duljina odgovarajućeg cjevovoda: 5 m; razlika razine: 0 m"]
["","","","","","(2) - Grijanje: unutarnja temperatura 20°CDB, vanjska temperatura 7°CDB, 6°CWB, odgovarajući cjevovod za radnu tvar: 5 m (vodoravno)","(2) - Grijanje: unutarnja temperatura 20°CDB, vanjska temperatura 7°CDB, 6°CWB, odgovarajući cjevovod za radnu tvar: 5 m (vodoravno)","(2) - Grijanje: unutarnja temperatura 20°CDB, vanjska temperatura 7°CDB, 6°CWB, odgovarajući cjevovod za radnu tvar: 5 m (vodoravno)","(2) - Grijanje: unutarnja temperatura 20°CDB, vanjska temperatura 7°CDB, 6°CWB, odgovarajući cjevovod za radnu tvar: 5 m (vodoravno)","(2) - Grijanje: unutarnja temperatura 20°CDB, vanjska temperatura 7°CDB, 6°CWB, odgovarajući cjevovod za radnu tvar: 5 m (vodoravno)"]
["","","","","","(3) - Vidi električne podatke na posebnim nacrtima","(3) - Vidi električne podatke na posebnim nacrtima","(3) - Vidi električne podatke na posebnim nacrtima","(3) - Vidi električne podatke na posebnim nacrtima","(3) - Vidi električne podatke na posebnim nacrtima"]