{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":17,"n_cols":11,"rows_kept":17,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXJ-MS / 3MXM-N"]
[]
[]
[]
[]
["","","","","FTXJ20MV1BS / FTXJ20MV1BS / 3MXM40N2V1B","FTXJ20MV1BS / FTXJ20MV1BS / FTXJ20MV1BS / 3MXM40N2V1B","FTXJ20MV1BW / FTXJ20MV1BS / 3MXM40N2V1B","FTXJ20MV1BS / FTXJ20MV1BS / FTXJ20MV1BS / 3MXM52N2V1B","FTXJ20MV1BS / FTXJ20MV1BS / 3MXM52N2V1B","FTXJ20MV1BS / FTXJ20MV1BS / 3MXM68N2V1B","FTXJ20MV1BS / FTXJ20MV1BS / FTXJ20MV1BS / 3MXM68N2V1B"]
["Cooling capacity","Nom.","","kW","4.00","4.00","4.0","5.20","4.00","4.00","6.00"]
["Nazivna učinkovitost","Annual energy consumption","","kWh","482","467","482","593","471","457","787"]
["","EER","","","4.15","4.28","4.15","4.38","4.25","4.38","3.81"]
["","COP","","","3.95","4.32","3.95","4.42","4.05","4.04","3.88"]
["","Direktiva o označivanju energetske učinkovitosti","Hlađenje","","A","A","A","A","A","A","A"]
["","","Grijanje","","A","A","A","A","A","A","A"]
["Učin grijanja","Nom.","","kW","4.60","4.60","4.60","6.80","6.80","6.50","7.80"]
["Napomene","","","","(1) - Nom. kapacitet hlađenja se temelji se na sljedećim parametrima: unutarnja temperatura: 27 °C DB, 19 °C WB, vanjska temperatura: 35 °C DB, odgovarajuće cijevi rashladnog sredstva: 5 m, razlika u visini: 0m.","","(1) - Nom.kapacitet hlađenja se temelji se na sljedećim paramerima: unutarnja temp.:27°CDB,19°CWB, vanjska temp.:35°CDB, odgovarajuće cijevi rashladnog sredstva:5m, razlika u visini:0m. Podaci za seriju standardne učinkovitosti. Koriste se tolerancije prema stand. Eurovent2015."]
["","","","","(2) - Nazivni učin grijanja zasnovani su na: unutarnja temperatura: 20°C DB, vanjska temperatura : 7°C DB, 6°C WB, odgovarajući cjevovod za radnu tvar: 5 m, razlika razine: 0 m.","","(2) - Nazivni učin grijanja zasnovani su na: unutarnja temperatura: 20°C DB, vanjska temperatura : 7°C DB, 6°C WB, odgovarajući cjevovod za radnu tvar: 5 m, razlika razine: 0 m."]
["","","","","(3) - Pogledajte odvojene nacrte za radno područje"]
["","","","","(4) - Vidi električne podatke na posebnim nacrtima"]