{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":33,"n_cols":10,"rows_kept":33,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXJ-MS / 3MXM-N"]
[]
[]
[]
[]
["","","","","FTXJ20MV1BS / FTXJ20MV1BS / FTXJ20MV1BS / 3MXM40N2V1B","FTXJ20MV1BS / FTXJ20MV1BS / 3MXM40N2V1B","FTXJ20MV1BS / FTXJ20MV1BS / FTXJ20MV1BS / 3MXM52N2V1B","FTXJ20MV1BS / FTXJ20MV1BS / 3MXM52N2V1B","FTXJ20MV1BS / FTXJ20MV1BS / 3MXM68N2V1B","FTXJ20MV1BS / FTXJ20MV1BS / FTXJ20MV1BS / 3MXM68N2V1B"]
["Učin hlađenja","Nom.","","kW","4.00","","5.20","4.00","4.00","6.00"]
["Nazivna učinkovitost","Godišnja potrošnja energije","","kWh","467","","593","471","457","787"]
["","EER","","","4.28","","4.38","4.25","4.38","3.81"]
["","COP","","","4.32","","4.42","4.05","4.04","3.88"]
["","Direktiva o označivanju energetske učinkovitosti","Hlađenje","","A","","A","A","A","A"]
["","","Grijanje","","A","","A","A","A","A"]
["Heating capacity","Nom.","","kW","4.60","","6.80","6.80","6.50","7.80"]
["Učin hlađenja","Nom.","","kW","","4.00"]
["Učin grijanja","Nom.","","kW","","4.60"]
["Nazivna učinkovitost","EER","","","","4.15"]
["","COP","","","","3.95"]
["","Godišnja potrošnja energije","","kWh","","482"]
["","Direktiva o označivanju energetske učinkovitosti","Hlađenje","","","A"]
["","","Grijanje","","","A"]
["Hlađenje prostora","Razred energetske učinkovitosti","","","","A++"]
["","Kapacitet","Pdesign","kW","","4.00"]
["","SEER","","","","7.62"]
["","Godišnja potrošnja energije","","kWh/a","","164"]
["Grijanje prostora (prosječna klima)","Razred energetske učinkovitosti","","","","A+"]
["","Kapacitet","Pdesign","kW","","4.80"]
["","SCOP/A","","","","4.11"]
["","Pdh kapacitet grijanja pri -10°","","kW","","3.58"]
["","Godišnja potrošnja energije","","kWh/a","","1632"]
["Napomene","","","","","(1) - Nom. kapacitet hlađenja se temelji se na sljedećim parametrima: unutarnja temperatura: 27 °C DB, 19 °C WB, vanjska temperatura: 35 °C DB, odgovarajuće cijevi rashladnog sredstva: 5 m, razlika u visini: 0m."]
["","","","","","(2) - Nazivni učin grijanja zasnovani su na: unutarnja temperatura: 20°C DB, vanjska temperatura : 7°C DB, 6°C WB, odgovarajući cjevovod za radnu tvar: 5 m, razlika razine: 0 m."]
["","","","","","(3) - Pogledajte odvojene nacrte za radno područje"]
["","","","","","(4) - Vidi električne podatke na posebnim nacrtima"]