{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":54,"n_cols":9,"rows_kept":54,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXJ-MW"]
[]
[]
[]
[]
["","","","","","FTXJ20MV1BW","FTXJ25MV1BW","FTXJ35MV1BW","FTXJ50MV1BW"]
["Ulazna struja","Hlađenje","","Nom.","kW","0.023","0.023","0.033","0.033"]
["","Grijanje","","Nom.","kW","0.031","0.033","0.042","0.043"]
["Kućište","Boja","","","","Bijelo","Bijelo","Bijelo","Bijelo"]
["Dimenzije","Uređaj","","Visina","mm","303","303","303","303"]
["","","","Širina","mm","998","998","998","998"]
["","","","Dubina","mm","212","212","212","212"]
["Težina","Uređaj","","","kg","12","12","12","12"]
["Ventilator","Količina zraka","Hlađenje","Visoko","m³/min","8.9","8.9","10.9","10.9"]
["","Protok zraka","Hlađenje","Srednji","m³/min","6.6","6.6","7.8","8.9"]
["","","","Nizak","m³/min","4.4","4.4","4.8","6.8"]
["","","","Tihi način rada","m³/min","2.6","2.6","2.9","3.6"]
["","","Grijanje","Visoko","m³/min","10.2","11.0","12.4","12.6"]
["","Protok zraka","Grijanje","Srednji","m³/min","8.4","8.6","9.6","10.5"]
["","","Grijanje","Nizak","m³/min","6.3","6.3","6.9","8.1"]
["","","","Tihi način rada","m³/min","3.8","3.8","4.1","5.0"]
["Zvučna snaga","Hlađenje","","","dBA","54","54","59","60"]
["","Grijanje","","","dBA","56","56","59","60"]
["Razina tlaka zvuka","Hlađenje","","Visoko","dBA","38","38","45","46"]
["Razina zvučnog tlaka","Hlađenje","","Srednji","dBA","32","32","34","40"]
["Razina tlaka zvuka","Hlađenje","","Nizak","dBA","25","25","26","35"]
["","","","Tihi način rada","dBA","19","19","20","25"]
["","Grijanje","","Visoko","dBA","40","41","45","47"]
["Razina zvučnog tlaka","Grijanje","","Srednji","dBA","34","34","37","41"]
["Razina tlaka zvuka","Grijanje","","Nizak","dBA","28","28","29","35"]
["","","","Tihi način rada","dBA","19","19","20","25"]
["Priključci cjevovoda","Tekućina","","VP","mm","6.35","6.35","6.35","6.35"]
["","Plin","","VP","mm","9.50","9.50","9.50","12.70"]
["","Odvod vode","","","","18","18","18","18"]
["Upravljački sustavi","Infrared remote control","","","","ARC466A9","ARC466A9","ARC466A9","ARC466A9"]
["Standardna dodatna oprema","Installation manual","","","","1","1","1","1"]
["","Wireless remote control","","","","1","1","1","1"]
["","Screw cover","","","","2","2","2","2"]
["","AAA dry-cell batteries","","","","2","2","2","2"]
["","Fixing screw for remote controller holder","","","","2","2","2","2"]
["","WLAN adapter kit","","","","1","1","1","1"]
["","Operation manual","","","","1","1","1","1"]
["","Titanium apatite deodorizing filter","","","","2","2","2","2"]
["","Fixing screws for mounting plate","","","","5","5","5","5"]
["","Indoor unit fixing screws","","","","2","2","2","2"]
["","Mounting plate","","","","1","1","1","1"]
["","Remote control holder","","","","1","1","1","1"]
["Napajanje","Naziv","","","","V1","V1","V1","V1"]
["","Faza","","","","1~","1~","1~","1~"]
["","Frekvencija","","","Hz","50","50","50","50"]
["","Napon","","","V","220-240","220-240","220-240","220-240"]
["Napomene","","","","","(1) - 220 V","(1) - 220 V","(1) - 220 V","(1) - 220 V"]
["","","","","","(2) - 230 V","(2) - 230 V","(2) - 230 V","(2) - 230 V"]
["","","","","","(3) - 240 V","(3) - 240 V","(3) - 240 V","(3) - 240 V"]