{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":24,"n_cols":6,"rows_kept":24,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXL-JV / RXL-M"]
[]
[]
[]
[]
["","","","","FTXL25J2V1B / RXL25M2V1B","FTXL35J2V1B / RXL35M2V1B"]
["Učin hlađenja","Min.","","kW","1.2","1.3"]
["","Maks.","","kW","3.4","3.8"]
["Piping connections","Tekućina","VP","mm","6.35","6.35"]
["","Plin","VP","mm","9.5","9.5"]
["","Drain","OD","mm","18","18"]
["Nazivna učinkovitost","Godišnja potrošnja energije","","kWh","400.5","570"]
["","EER","","","3.12","3.07"]
["","COP","","","4.43","4.21"]
["","Direktiva o označivanju energetske učinkovitosti","Hlađenje","","B","B"]
["","","Grijanje","","A","A"]
["Učin grijanja","Min.","","kW","1.1","1.2"]
["","Maks.","","kW","5.5","6.0"]
["Napomene","","","","(1) - Za minimalni nazivni učin, ventilator unutarnje jedinice postavite na SL izvod","(1) - Za minimalni nazivni učin, ventilator unutarnje jedinice postavite na SL izvod"]
["","","","","(2) - 220 V","(2) - 220 V"]
["","","","","(3) - 230 V","(3) - 230 V"]
["","","","","(4) - 240 V","(4) - 240 V"]
["","","","","(5) - EER/COP prema Eurovent 2012, za korištenje samo izvan EU","(5) - EER/COP prema Eurovent 2012, za korištenje samo izvan EU"]
["","","","","(6) - Nazivna učinkovitost: hlađenje na 35°/27° nazivnog opterećenja, grijanje na 7°/20° nazivnog opterećenja","(6) - Nazivna učinkovitost: hlađenje na 35°/27° nazivnog opterećenja, grijanje na 7°/20° nazivnog opterećenja"]