{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":43,"n_cols":6,"rows_kept":43,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXLS-K3"]
[]
[]
[]
[]
["","","","","FTXLS25K3V1B","FTXLS35K3V1B"]
["Razina tlaka zvuka","Grijanje","Visoko","dBA","47","47"]
["","","Tihi način rada","dBA","19","19"]
["","","Nizak","dBA","23","23"]
["","Hlađenje","Tihi način rada","dBA","21","21"]
["","","Nizak","dBA","33","33"]
["","","Visoko","dBA","45","45"]
["","","Nom.","dBA","37","36"]
["","Hlađenje","Nom.","dBA","39","39"]
["Standardna dodatna oprema","Priručnik za instalaciju","","","1","1"]
["","Radni priručnik","","","1","1"]
["","Infracrveno daljinsko upravljanje","","","1","1"]
["","Baterije","","","2","2"]
["","Držač daljinskog upravljača","","","1","1"]
["","Montažna ploča","","","1","1"]
["","Fotokatalitički filtar za pročišćavanje zraka iz titan-apatita","","","2","2"]
["","Učvrsni vijak unutarnje jedinice","","","2","2"]
["Upravljački sustavi","Infrared remote control","","","ARC466A9","ARC466A9"]
["Priključci cjevovoda","Tekućina","VP","mm","6.35","6.35"]
["","Plin","VP","mm","9.5","9.5"]
["","Odvod vode","","","18","18"]
["Ulazna struja","Hlađenje","Nom.","kW","0.024 (2), 0.024 (3), 0.024 (4)","0.024 (2), 0.024 (3), 0.024 (4)"]
["","Grijanje","Nom.","kW","0.030 (2), 0.030 (3), 0.030 (4)","0.030 (2), 0.030 (3), 0.030 (4)"]
["Razina zvučne snage","Hlađenje","","dBA","59","59"]
["","Grijanje","","dBA","62","62"]
["Dimenzije","Jedinica","Širina","mm","900","900"]
["","","Dubina","mm","215","215"]
["","","Visina","mm","298","298"]
["Kućište","Colour","","","Bijelo","Bijelo"]
["Težina","Uređaj","","kg","12","12"]
["Power supply","Phase","","","1~","1~"]
["","Frekvencija","","Hz","50","50"]
["","Naziv","","","V1","V1"]
["","Napon","","V","220-240","220-240"]
["Napomene","","","","(1) - Kada se spaja s vanjskom jedinicom za više sustava, pogledajte tehničke podatke vanjske jedinice za više sustava koju treba spojiti.","(1) - Kada se spaja s vanjskom jedinicom za više sustava, pogledajte tehničke podatke vanjske jedinice za više sustava koju treba spojiti."]
["","","","","(2) - 220 V","(2) - 220 V"]
["","","","","(3) - 230 V","(3) - 230 V"]
["","","","","(4) - 240 V","(4) - 240 V"]