{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":55,"n_cols":7,"rows_kept":55,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXTM-A"]
[]
[]
[]
[]
["","","","","","FTXTM30A2V1B","FTXTM40A2V1B"]
["Ulazna struja","Hlađenje","","Nom.","kW","0.029","0.053"]
["","Grijanje","","Nom.","kW","0.024","0.06"]
["Kućište","Boja","","","","Bijelo","Bijelo"]
["Dimenzije","Uređaj","","Visina","mm","298","298"]
["","","","Širina","mm","804","997"]
["","","","Dubina","mm","252","292"]
["Težina","Uređaj","","","kg","12","15"]
["Ventilator","Količina zraka","Hlađenje","Visoko","m³/min","13.2","15.1"]
["","Protok zraka","Hlađenje","Srednji","m³/min","8.1","9.2"]
["","","","Nizak","m³/min","5.6","5.6"]
["","","","Tihi način rada","m³/min","4.8","4.8"]
["","","Grijanje","Visoko","m³/min","11.7","17"]
["","Protok zraka","Grijanje","Srednji","m³/min","7.7","10"]
["","","Grijanje","Nizak","m³/min","5.6","6"]
["","","","Tihi način rada","m³/min","4.7","5.1"]
["Zvučna snaga","Hlađenje","","","dBA","60","60"]
["","Grijanje","","","dBA","59","60"]
["Razina tlaka zvuka","Hlađenje","","Visoko","dBA","45","46"]
["Razina zvučnog tlaka","Hlađenje","","Srednji","dBA","33","32"]
["Razina tlaka zvuka","Hlađenje","","Nizak","dBA","25","24"]
["","","","Tihi način rada","dBA","21","20"]
["","Grijanje","","Visoko","dBA","43","46"]
["Razina zvučnog tlaka","Grijanje","","Srednji","dBA","31","31"]
["Razina tlaka zvuka","Grijanje","","Nizak","dBA","22","22"]
["","","","Tihi način rada","dBA","19","19"]
["Radna tvar","GWP","","","","675","675"]
["Priključci cjevovoda","Tekućina","","VP","mm","6.35","6.35"]
["","Plin","","VP","mm","9.5","9.5"]
["","Odvod vode","","","","18","18"]
["Upravljački sustavi","Infracrveno daljinsko upravljanje","","","","ARC466A83","ARC466A83"]
["Standardna dodatna oprema","FTXTM30A2V1B","","","","1"]
["","Installation manual","","","","1","1"]
["","Wireless remote control","","","","1","1"]
["","Screw cover","","","","2","2"]
["","AAA dry-cell batteries","","","","2","2"]
["","General safety precautions","","","","1","1"]
["","Operation manual","","","","1","1"]
["","Titanium apatite deodorizing filter","","","","1","1"]
["","Silver particle filter","","","","1","1"]
["","Remote control holder","","","","1","1"]
["","Screw bag","","","","1","1"]
["Napajanje","Naziv","","","","V1","V1"]
["","Faza","","","","1~","1~"]
["","Frekvencija","","","Hz","50","50"]
["","Napon","","","V","220-240","220-240"]
["Napomene","","","","","(1) - Hlađenje: unutarnja temperatura 27°CDB, 19°CWB; vanjska temperatura 35°CDB; 24°CWB, duljina odgovarajućeg cjevovoda: 5 m","(1) - Hlađenje: unutarnja temperatura 27°CDB, 19°CWB; vanjska temperatura 35°CDB; 24°CWB, duljina odgovarajućeg cjevovoda: 5 m"]
["","","","","","(2) - Grijanje: unutarnja temperatura 20°CDB, vanjska temperatura 7°CDB, 6°CWB, odgovarajući cjevovod za radnu tvar: 5 m","(2) - Grijanje: unutarnja temperatura 20°CDB, vanjska temperatura 7°CDB, 6°CWB, odgovarajući cjevovod za radnu tvar: 5 m"]
["","","","","","(3) - Vidi električne podatke na posebnim nacrtima","(3) - Vidi električne podatke na posebnim nacrtima"]
["Standardna dodatna oprema","FTXTM40A2V1B","","","","","1"]