{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":47,"n_cols":7,"rows_kept":47,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXTM-S"]
[]
[]
[]
[]
["","","","","","FTXTM30S2V1B","FTXTM40S2V1B"]
["Ulazna struja","Hlađenje","","Nom.","kW","0.035","0.053"]
["","Grijanje","","Nom.","kW","0.039","0.06"]
["Kućište","Boja","","","","Bijelo","Bijelo"]
["Dimenzije","Uređaj","","Visina","mm","295","299"]
["","","","Širina","mm","778","998"]
["","","","Dubina","mm","272","292"]
["Težina","Uređaj","","","kg","10","15"]
["Ventilator","Količina zraka","Hlađenje","Visoko","m³/min","11.5","15.1"]
["","Protok zraka","Hlađenje","Srednji","m³/min","7.5","9.2"]
["","","","Nizak","m³/min","5.2","5.6"]
["","","","Tihi način rada","m³/min","4.2","4.8"]
["","","Grijanje","Visoko","m³/min","11.6","17"]
["","Protok zraka","Grijanje","Srednji","m³/min","7.3","10"]
["","","Grijanje","Nizak","m³/min","4.7","6"]
["","","","Tihi način rada","m³/min","4","5.1"]
["Zvučna snaga","Hlađenje","","","dBA","60","60"]
["","Grijanje","","","dBA","60","60"]
["Razina tlaka zvuka","Hlađenje","","Visoko","dBA","45","46"]
["Razina zvučnog tlaka","Hlađenje","","Srednji","dBA","33","32"]
["Razina tlaka zvuka","Hlađenje","","Nizak","dBA","25","24"]
["","","","Tihi način rada","dBA","21","20"]
["","Grijanje","","Visoko","dBA","45","46"]
["Razina zvučnog tlaka","Grijanje","","Srednji","dBA","31","31"]
["Razina tlaka zvuka","Grijanje","","Nizak","dBA","22","22"]
["","","","Tihi način rada","dBA","19","19"]
["Radna tvar","GWP","","","","675","675"]
["Priključci cjevovoda","Tekućina","","VP","mm","6.35","6.35"]
["","Plin","","VP","mm","9.5","9.5"]
["","Odvod vode","","","","18","18"]
["Upravljački sustavi","Infracrveno daljinsko upravljanje","","","","ARC466A83","ARC466A83"]
["","Žično daljinsko upravljanje","","","","BRC073A1","BRC073A1"]
["Standardna dodatna oprema","Installation manual","","","","1","1"]
["","Wireless remote control","","","","1","1"]
["","AAA dry-cell batteries","","","","2","2"]
["","General safety precautions","","","","1","1"]
["","Silver particle filter","","","","1","1"]
["","Remote control holder","","","","1","1"]
["","Screw bag","","","","1","1"]
["Napajanje","Faza","","","","1~","1~"]
["","Frekvencija","","","Hz","50","50"]
["","Napon","","","V","220-240","220-240"]