{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":55,"n_cols":7,"rows_kept":55,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXTP-A"]
[]
[]
[]
[]
["","","","","","FTXTP25A5V1B","FTXTP35A5V1B"]
["Ulazna struja","Hlađenje","","Nom.","kW","0.032","0.032"]
["","Grijanje","","Nom.","kW","0.032","0.032"]
["Kućište","Boja","","","","Bijelo","Bijelo"]
["Dimenzije","Uređaj","","Visina","mm","286","286"]
["","","","Širina","mm","770","770"]
["","","","Dubina","mm","225","225"]
["Težina","Uređaj","","","kg","9","9"]
["Ventilator","Količina zraka","Hlađenje","Visoko","m³/min","11","11"]
["","Protok zraka","Hlađenje","Srednji","m³/min","7.9","7.9"]
["","","","Nizak","m³/min","5","5"]
["","","","Tihi način rada","m³/min","3.7","3.7"]
["","","Grijanje","Visoko","m³/min","10.5","10.5"]
["","Protok zraka","Grijanje","Srednji","m³/min","9","9"]
["","","Grijanje","Nizak","m³/min","5.5","5.5"]
["","","","Tihi način rada","m³/min","4.4","4.4"]
["Zvučna snaga","Hlađenje","","","dBA","58","58"]
["","Grijanje","","","dBA","58","58"]
["Razina tlaka zvuka","Hlađenje","","Visoko","dBA","43","43"]
["Razina zvučnog tlaka","Hlađenje","","Srednji","dBA","35","35"]
["Razina tlaka zvuka","Hlađenje","","Nizak","dBA","26","26"]
["","","","Tihi način rada","dBA","21","21"]
["","Grijanje","","Visoko","dBA","43","43"]
["Razina zvučnog tlaka","Grijanje","","Srednji","dBA","35","35"]
["Razina tlaka zvuka","Grijanje","","Nizak","dBA","26","26"]
["","","","Tihi način rada","dBA","21","21"]
["Radna tvar","GWP","","","","675","675"]
["Priključci cjevovoda","Tekućina","","VP","mm","6.35","6.35"]
["","Plin","","VP","mm","9.5","9.5"]
["","Odvod vode","","","","18","18"]
["Control systems","Infracrveno daljinsko upravljanje","","","","ARC480A78","ARC480A78"]
["Standardna dodatna oprema","FTXTP25A5V1B","","","","1"]
["","Installation manual","","","","1","1"]
["","Wireless remote control","","","","1","1"]
["","Screw cover","","","","2","2"]
["","AAA dry-cell batteries","","","","2","2"]
["","General safety precautions","","","","1","1"]
["","Operation manual","","","","1","1"]
["","Titanium apatite deodorizing filter","","","","1","1"]
["","Silver particle filter","","","","1","1"]
["","Remote control holder","","","","1","1"]
["","Screw bag","","","","1","1"]
["Napajanje","Naziv","","","","V1","V1"]
["","Faza","","","","1~","1~"]
["","Frekvencija","","","Hz","50","50"]
["","Napon","","","V","220-240","220-240"]
["Napomene","","","","","(1) - Hlađenje: unutarnja temperatura 27°CDB, 19°CWB; vanjska temperatura 35°CDB; 24°CWB, duljina odgovarajućeg cjevovoda: 5 m","(1) - Hlađenje: unutarnja temperatura 27°CDB, 19°CWB; vanjska temperatura 35°CDB; 24°CWB, duljina odgovarajućeg cjevovoda: 5 m"]
["","","","","","(2) - Grijanje: unutarnja temperatura 20°CDB, vanjska temperatura 7°CDB, 6°CWB, odgovarajući cjevovod za radnu tvar: 5 m","(2) - Grijanje: unutarnja temperatura 20°CDB, vanjska temperatura 7°CDB, 6°CWB, odgovarajući cjevovod za radnu tvar: 5 m"]
["","","","","","(3) - Vidi električne podatke na posebnim nacrtima","(3) - Vidi električne podatke na posebnim nacrtima"]
["Standardna dodatna oprema","FTXTP35A5V1B","","","","","1"]