{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":23,"n_cols":10,"rows_kept":23,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FUQ-C / RZQG-L(8)Y1"]
[]
[]
[]
[]
["","","","","FUQ100CVEB / RZQG71L8Y1B","FUQ71CVEB / RZQG71L8Y1B","FUQ100CVEB / RZQG100L8Y1B","FUQ71CVEB / FUQ71CVEB / RZQG100L8Y1B","FUQ125CVEB / RZQG125L8Y1B","FUQ71CVEB / FUQ71CVEB / RZQG125L8Y1B"]
["Učin hlađenja","Nom.","","kW","","6.8","9.5","","12.0"]
["Hlađenje prostora","SEER","","","6.50","6.42","6.11","5.10","5.61","5.10"]
["","Godišnja potrošnja energije","","kWh/a","367","371","545","652","749","824"]
["","Kapacitet","Pdesign","kW","6.80","6.80","9.5","9.50","12","12.00"]
["","Razred energetske učinkovitosti","","","A++","A++","A++","B","A+","B"]
["Grijanje prostora (prosječna klima)","Kapacitet","Pdesign","kW","7.60","7.60","11.3","11.30","14.13","12.71"]
["","SCOP/A","","","4.20","4.20","4.5","3.80","4.44","3.80"]
["","Razred energetske učinkovitosti","","","A+","A+","A+","A","A+","A"]
["","Godišnja potrošnja energije","","kWh/a","2,534","2,534","3,516","4,164","4,456","4,683"]
["Nazivna učinkovitost","Godišnja potrošnja energije","","kWh","","840","1,230","","1,770"]
["","EER","","","","4.05","3.86","","3.39"]
["","COP","","","","4.08","3.95","","3.42"]
["","Direktiva o označivanju energetske učinkovitosti","Hlađenje","","","A","A","","A"]
["","","Grijanje","","","A","A","","B"]
["Učin grijanja","Nom.","","kW","","7.5","10.8","","13.5"]
["Napomene","","","","","(1) - Godišnja potrošnja energije u skladu je s direktivom oznake energetske učinkovitosti 2002/31/EC","(1) - EER/COP prema Eurovent 2012, za korištenje samo izvan EU","","(1) - EER/COP prema Eurovent 2012, za korištenje samo izvan EU"]
["","","","","","(2) - SEER i SCOP su u skladu s EN 14825","(2) - Nazivna učinkovitost: hlađenje na 35°/27° nazivnog opterećenja, grijanje na 7°/20° nazivnog opterećenja","","(2) - Nazivna učinkovitost: hlađenje na 35°/27° nazivnog opterećenja, grijanje na 7°/20° nazivnog opterećenja"]