{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":51,"n_cols":8,"rows_kept":51,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FVXM-A9"]
[]
[]
[]
[]
["","","","","","FVXM25A3V1B9","FVXM35A3V1B9","FVXM50A3V1B9"]
["Ulazna struja","Hlađenje","","Nom.","kW","0.02","0.02","0.03"]
["","Grijanje","","Nom.","kW","0.02","0.03","0.03"]
["Kućište","Boja","","","","Bijelo","Bijelo","Bijelo"]
["Dimenzije","Uređaj","","Visina","mm","600","600","600"]
["","","","Širina","mm","750","750","750"]
["","","","Dubina","mm","238","238","238"]
["Težina","Uređaj","","","kg","17","17","17"]
["Ventilator","Količina zraka","Hlađenje","Visoko","m³/min","8.7","9.2","11.6"]
["","Protok zraka","Hlađenje","Srednji","m³/min","7","7","9"]
["","","","Nizak","m³/min","4.9","4.9","6.6"]
["","","","Tihi način rada","m³/min","4.1","4.1","5.4"]
["","","Grijanje","Visoko","m³/min","9.2","9.8","12.8"]
["","Protok zraka","Grijanje","Srednji","m³/min","7.2","7.2","10"]
["","","Grijanje","Nizak","m³/min","5.6","5.6","8.4"]
["","","","Tihi način rada","m³/min","4.1","4.1","5.9"]
["Zvučna snaga","Hlađenje","","","dBA","52","53","61"]
["","Grijanje","","","dBA","52","53","62"]
["Razina tlaka zvuka","Hlađenje","","Visoko","dBA","38","39","44"]
["Razina zvučnog tlaka","Hlađenje","","Srednji","dBA","32","32","38"]
["Razina tlaka zvuka","Hlađenje","","Nizak","dBA","25","25","31"]
["","","","Tihi način rada","dBA","20","20","27"]
["","Grijanje","","Visoko","dBA","38","39","46"]
["Razina zvučnog tlaka","Grijanje","","Srednji","dBA","32","32","40"]
["Razina tlaka zvuka","Grijanje","","Nizak","dBA","25","25","35"]
["","","","Tihi način rada","dBA","19","19","29"]
["Radna tvar","GWP","","","","675","675","675"]
["Priključci cjevovoda","Tekućina","","VP","mm","6.4","6.4","6.4"]
["","Plin","","VP","mm","9.5","9.5","12.7"]
["","Odvod vode","","","","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)"]
["Upravljački sustavi","Infracrveno daljinsko upravljanje","","","","ARC466A66","ARC466A66","ARC466A66"]
["","Žično daljinsko upravljanje","","","","BRC073A1","BRC073A1","BRC073A1"]
["Napajanje","Faza","","","","1~","1~","1~"]
["","Frekvencija","","","Hz","50","50","50"]
["","Napon","","","V","220-240","220-240","220-240"]
["Standardna dodatna oprema","Installation manual","","","","1","1","1"]
["","Wireless remote control","","","","1","1","1"]
["","AAA dry-cell batteries","","","","2","2","2"]
["","General safety precautions","","","","1","1","1"]
["","Operation manual","","","","1","1","1"]
["","Titanium apatite deodorizing filter","","","","2","2","2"]
["","Remote control holder","","","","1","1","1"]
["","Screw bag","","","","1","1","1"]
["Raspon energetske učinkovitosti","","","","","A+++ ~ D"]
["Napomene","","","","","(1) - Hlađenje: unutarnja temperatura 27°CDB, 19°CWB; vanjska temperatura 35°CDB; 24°CWB, duljina odgovarajućeg cjevovoda: 5 m"]
["","","","","","(2) - Grijanje: unutarnja temperatura 20°CDB, vanjska temperatura 7°CDB, 6°CWB, odgovarajući cjevovod za radnu tvar: 5 m"]