{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":48,"n_cols":6,"rows_kept":48,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FVXTM-A"]
[]
[]
[]
[]
["","","","","","FVXTM30A3V1B"]
["Ulazna struja","Hlađenje","","Nom.","kW","0.02"]
["","Grijanje","","Nom.","kW","0.03"]
["Kućište","Boja","","","","Bijelo"]
["Dimenzije","Uređaj","","Visina","mm","600"]
["","","","Širina","mm","750"]
["","","","Dubina","mm","238"]
["Težina","Uređaj","","","kg","17"]
["Ventilator","Količina zraka","Hlađenje","Visoko","m³/min","9"]
["","Protok zraka","Hlađenje","Srednji","m³/min","6.7"]
["","","","Nizak","m³/min","4.8"]
["","","","Tihi način rada","m³/min","4"]
["","","Grijanje","Visoko","m³/min","9.4"]
["","Protok zraka","Grijanje","Srednji","m³/min","6.8"]
["","","Grijanje","Nizak","m³/min","5.3"]
["","","","Tihi način rada","m³/min","4"]
["Zvučna snaga","Hlađenje","","","dBA","53"]
["","Grijanje","","","dBA","53"]
["Razina tlaka zvuka","Hlađenje","","Visoko","dBA","39"]
["Razina zvučnog tlaka","Hlađenje","","Srednji","dBA","32"]
["Razina tlaka zvuka","Hlađenje","","Nizak","dBA","25"]
["","","","Tihi način rada","dBA","20"]
["","Grijanje","","Visoko","dBA","39"]
["Razina zvučnog tlaka","Grijanje","","Srednji","dBA","32"]
["Razina tlaka zvuka","Grijanje","","Nizak","dBA","25"]
["","","","Tihi način rada","dBA","19"]
["Radna tvar","GWP","","","","675"]
["Priključci cjevovoda","Tekućina","","VP","mm","6.35"]
["","Plin","","VP","mm","9.5"]
["","Odvod vode","","","","VP20 (I.D. 20/O.D. 26)"]
["Control systems","Infrared remote control","","","","ARC466A66"]
["Upravljački sustavi","Žično daljinsko upravljanje","","","","BRC073A1"]
["Standardna dodatna oprema","Installation manual","","","","1"]
["","Wireless remote control","","","","1"]
["","AAA dry-cell batteries","","","","2"]
["","General safety precautions","","","","1"]
["","Operation manual","","","","1"]
["","Titanium apatite deodorizing filter","","","","2"]
["","Remote control holder","","","","1"]
["","Screw bag","","","","2"]
["Napajanje","Faza","","","","1~"]
["","Frekvencija","","","Hz","50"]
["","Napon","","","V","220-240"]