{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":48,"n_cols":11,"rows_kept":48,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FXAA-A"]
[]
[]
[]
[]
["","","","","FXAA15AUV1B","FXAA20AUV1B","FXAA25AUV1B","FXAA32AUV1B","FXAA40AUV1B","FXAA50AUV1B","FXAA63AUV1B"]
["Razina tlaka zvuka","Grijanje","Na većoj brzini ventilatora","dBA","33.0","34.0","36.0","38.5","38.0","42.0","47.0"]
["","","Na niskoj brzini ventilatora","dBA","28.5","28.5","28.5","28.5","33.5","35.5","38.5"]
["","","Na srednjoj brzini ventilatora","dBA","31.0","31.5","32.5","33.5","36.0","39.0","43.0"]
["","Hlađenje","Na niskoj brzini ventilatora","dBA","28.5","28.5","28.5","28.5","33.5","35.5","38.5"]
["","","Na većoj brzini ventilatora","dBA","32.0","33.0","35.0","37.5","37.0","41.0","46.5"]
["","","Na srednjoj brzini ventilatora","dBA","30.5","31.0","32.0","33.0","35.5","38.5","42.5"]
["Standardna dodatna oprema","Priručnik za instalaciju i rukovanje","","","1","1","1","1","1","1","1"]
["","Instalacijska ploča","","","1","1","1","1","1","1","1"]
["","Uzorak za montažu","","","1","1","1","1","1","1","1"]
["","Vreća s vijcima","","","1","1","1","1","1","1","1"]
["","Materijal stezaljke žice","","","4","4","4","4","4","4","4"]
["","Izolirana grijaća traka","","","1","1","1","1","1","1","1"]
["","Opće mjere sigurnosti","","","1","1","1","1","1","1","1"]
["Radna tvar","GWP","","","675.0","675.0","675.0","675.0","675.0","675.0","675.0"]
["","Tip","","","R-32","R-32","R-32","R-32","R-32","R-32","R-32"]
["Učin hlađenja","Ukupan učin","Na većoj brzini ventilatora","kW","1.7","2.2","2.8","3.6","4.5","5.6","7.1"]
["Priključci cjevovoda","Tekućina","VP","mm","6","6","6","6","6","6","6"]
["","","Tip","","Konusna spojnica","Konusna spojnica","Konusna spojnica","Konusna spojnica","Konusna spojnica","Konusna spojnica","Konusna spojnica"]
["","Plin","VP","mm","9.52","9.52","9.52","9.52","12.70","12.70","12.70"]
["","","Tip","","Konusna spojnica","Konusna spojnica","Konusna spojnica","Konusna spojnica","Konusna spojnica","Konusna spojnica","Konusna spojnica"]
["","Drain","","","VP13 (I.D. 15/O.D. 18)","VP13 (I.D. 15/O.D. 18)","VP13 (I.D. 15/O.D. 18)","VP13 (I.D. 15/O.D. 18)","VP13 (I.D. 15/O.D. 18)","VP13 (I.D. 15/O.D. 18)","VP13 (I.D. 15/O.D. 18)"]
["Sound power level","Hlađenje","Na većoj brzini ventilatora","dBA","51.0","52.0","53.0","55.0","55.0","58.0","63.0"]
["Zračni filtar","Type","","","Uklonjivo / perivo","Uklonjivo / perivo","Uklonjivo / perivo","Uklonjivo / perivo","Uklonjivo / perivo","Uklonjivo / perivo","Uklonjivo / perivo"]
["Dimenzije","Uređaj","Širina","mm","795","795","795","795","1,050","1,050","1,050"]
["","","Dubina","mm","266","266","266","266","269","269","269"]
["","","Visina","mm","290","290","290","290","290","290","290"]
["Casing","Colour","","","Bijelo","Bijelo","Bijelo","Bijelo","Bijelo","Bijelo","Bijelo"]
["Težina","Uređaj","","kg","12","12","12","12","15","15","15"]
["Učin grijanja","Ukupni učin","Na većoj brzini ventilatora","kW","1.9","2.5","3.2","4.0","5.0","6.3","8.0"]
["Power supply","Phase","","","1~","1~","1~","1~","1~","1~","1~"]
["","Frekvencija","","Hz","50","50","50","50","50","50","50"]
["","Naziv","","","V1","V1","V1","V1","V1","V1","V1"]
["","Napon","","V","220-240","220-240","220-240","220-240","220-240","220-240","220-240"]
["Napomene","","","","(1) - Hlađenje: unutarnja temperatura 27°CDB, 19,0°CWB; vanjska temperatura 35°CDB","(1) - Hlađenje: unutarnja temperatura 27°CDB, 19,0°CWB; vanjska temperatura 35°CDB","(1) - Hlađenje: unutarnja temperatura 27°CDB, 19,0°CWB; vanjska temperatura 35°CDB","(1) - Hlađenje: unutarnja temperatura 27°CDB, 19,0°CWB; vanjska temperatura 35°CDB","(1) - Hlađenje: unutarnja temperatura 27°CDB, 19,0°CWB; vanjska temperatura 35°CDB","(1) - Hlađenje: unutarnja temperatura 27°CDB, 19,0°CWB; vanjska temperatura 35°CDB","(1) - Hlađenje: unutarnja temperatura 27°CDB, 19,0°CWB; vanjska temperatura 35°CDB"]
["","","","","(2) - Grijanje: unutarnja temperatura 20°CDB, vanjska temperatura 7°CDB, 6°CWB","(2) - Grijanje: unutarnja temperatura 20°CDB, vanjska temperatura 7°CDB, 6°CWB","(2) - Grijanje: unutarnja temperatura 20°CDB, vanjska temperatura 7°CDB, 6°CWB","(2) - Grijanje: unutarnja temperatura 20°CDB, vanjska temperatura 7°CDB, 6°CWB","(2) - Grijanje: unutarnja temperatura 20°CDB, vanjska temperatura 7°CDB, 6°CWB","(2) - Grijanje: unutarnja temperatura 20°CDB, vanjska temperatura 7°CDB, 6°CWB","(2) - Grijanje: unutarnja temperatura 20°CDB, vanjska temperatura 7°CDB, 6°CWB"]
["","","","","(3) - Razina jačine zvuka apsolutna je vrijednost koja označava snagu koju generira izvor zvuka.","(3) - Razina jačine zvuka apsolutna je vrijednost koja označava snagu koju generira izvor zvuka.","(3) - Razina jačine zvuka apsolutna je vrijednost koja označava snagu koju generira izvor zvuka.","(3) - Razina jačine zvuka apsolutna je vrijednost koja označava snagu koju generira izvor zvuka.","(3) - Razina jačine zvuka apsolutna je vrijednost koja označava snagu koju generira izvor zvuka.","(3) - Razina jačine zvuka apsolutna je vrijednost koja označava snagu koju generira izvor zvuka.","(3) - Razina jačine zvuka apsolutna je vrijednost koja označava snagu koju generira izvor zvuka."]
["","","","","(4) - Raspon napona: jedinice su prikladne za uporabu na električnim sustavima pri kojima napon kojim se opskrbljuje terminal jedinice nije ispod ili iznad navedenih granica raspona.","(4) - Raspon napona: jedinice su prikladne za uporabu na električnim sustavima pri kojima napon kojim se opskrbljuje terminal jedinice nije ispod ili iznad navedenih granica raspona.","(4) - Raspon napona: jedinice su prikladne za uporabu na električnim sustavima pri kojima napon kojim se opskrbljuje terminal jedinice nije ispod ili iznad navedenih granica raspona.","(4) - Raspon napona: jedinice su prikladne za uporabu na električnim sustavima pri kojima napon kojim se opskrbljuje terminal jedinice nije ispod ili iznad navedenih granica raspona.","(4) - Raspon napona: jedinice su prikladne za uporabu na električnim sustavima pri kojima napon kojim se opskrbljuje terminal jedinice nije ispod ili iznad navedenih granica raspona.","(4) - Raspon napona: jedinice su prikladne za uporabu na električnim sustavima pri kojima napon kojim se opskrbljuje terminal jedinice nije ispod ili iznad navedenih granica raspona.","(4) - Raspon napona: jedinice su prikladne za uporabu na električnim sustavima pri kojima napon kojim se opskrbljuje terminal jedinice nije ispod ili iznad navedenih granica raspona."]
["","","","","(5) - Maksimalno dopušteno odstupanje napona između faza je 2%","(5) - Maksimalno dopušteno odstupanje napona između faza je 2%","(5) - Maksimalno dopušteno odstupanje napona između faza je 2%","(5) - Maksimalno dopušteno odstupanje napona između faza je 2%","(5) - Maksimalno dopušteno odstupanje napona između faza je 2%","(5) - Maksimalno dopušteno odstupanje napona između faza je 2%","(5) - Maksimalno dopušteno odstupanje napona između faza je 2%"]
["","","","","(6) - MCA/MFA: MCA = 1.1 x FLA","(6) - MCA/MFA: MCA = 1.1 x FLA","(6) - MCA/MFA: MCA = 1.1 x FLA","(6) - MCA/MFA: MCA = 1.1 x FLA","(6) - MCA/MFA: MCA = 1.1 x FLA","(6) - MCA/MFA: MCA = 1.1 x FLA","(6) - MCA/MFA: MCA = 1.1 x FLA"]
["","","","","(7) - Umjesto osigurača koristite prekidač strujnog kruga","(7) - Umjesto osigurača koristite prekidač strujnog kruga","(7) - Umjesto osigurača koristite prekidač strujnog kruga","(7) - Umjesto osigurača koristite prekidač strujnog kruga","(7) - Umjesto osigurača koristite prekidač strujnog kruga","(7) - Umjesto osigurača koristite prekidač strujnog kruga","(7) - Umjesto osigurača koristite prekidač strujnog kruga"]
["","","","","(8) - Odaberite veličinu žice zasnovanu na vrijednosti MCA","(8) - Odaberite veličinu žice zasnovanu na vrijednosti MCA","(8) - Odaberite veličinu žice zasnovanu na vrijednosti MCA","(8) - Odaberite veličinu žice zasnovanu na vrijednosti MCA","(8) - Odaberite veličinu žice zasnovanu na vrijednosti MCA","(8) - Odaberite veličinu žice zasnovanu na vrijednosti MCA","(8) - Odaberite veličinu žice zasnovanu na vrijednosti MCA"]
["","","","","(9) - Sadrži fluorovodične stakleničke plinove","(9) - Sadrži fluorovodične stakleničke plinove","(9) - Sadrži fluorovodične stakleničke plinove","(9) - Sadrži fluorovodične stakleničke plinove","(9) - Sadrži fluorovodične stakleničke plinove","(9) - Sadrži fluorovodične stakleničke plinove","(9) - Sadrži fluorovodične stakleničke plinove"]