{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":25,"n_cols":11,"rows_kept":25,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RXC-D"]
[]
[]
[]
[]
["","","","","","RXC20DV1B","RXC25DV1B","RXC35DV1B","RXC50DV1B","RXC60DV1B","RXC71DV1B"]
["Dimenzije","Uređaj","","Visina","mm","550","550","550","615","615","695"]
["","","","Širina","mm","658","658","658","845","845","930"]
["","","","Dubina","mm","273","273","273","300","300","350"]
["Težina","Uređaj","","","kg","24.0","24.0","26.0","39.0","39.0","45.0"]
["Kompresor","Tip","","","","Hermetički swing","Hermetički swing","Hermetički swing","Hermetički swing","Hermetički swing","Hermetički swing"]
["Radno područje","Hlađenje","Ambijent:","Min.","°CDB","10","10","10","-10","-10","-10"]
["","","","Maks.","°CDB","46","46","46","46","46","46"]
["","Grijanje","Ambijent:","Min.","°CWB","-15","-15","-15","-15","-15","-15"]
["","","","Maks.","°CWB","18","18","18","18","18","18"]
["Sound power level","Hlađenje","","","dBA","58","58","60","65","66","69"]
["Razina tlaka zvuka","Hlađenje","","Visoko","dBA","45","45","46","51","54","54"]
["Radna tvar","Tip","","","","R-32","R-32","R-32","R-32","R-32","R-32"]
["","Punjenje","","","kg","0.550","0.550","0.750","1.00","1.10","1.15"]
["","GWP","","","","675.0","675.0","675.0","675.0","675.0","675.0"]
["Priključci cjevovoda","Punjenje dodatne radne tvari","","","kg/m","0.017 (za duljinu cjevovoda koja premašuje 7,5m)","0.017 (za duljinu cjevovoda koja premašuje 7,5m)","0.017 (za duljinu cjevovoda koja premašuje 7,5m)","0.017 (za duljinu cjevovoda koja premašuje 7,5m)","0.017 (za duljinu cjevovoda koja premašuje 7,5m)","0.017 (za duljinu cjevovoda koja premašuje 7,5m)"]
["","razlika u razini","IU - OU","Maks.","m","15.0","15.0","15.0","20.0","20.0","20.0"]
["Power supply","Faza","","","","1~","1~","1~","1~","1~","1~"]
["","Frekvencija","","","Hz","50","50","50","50","50","50"]
["","Napon","","","V","220-240","220-240","220-240","220-240","220-240","220-240"]