{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":32,"n_cols":7,"rows_kept":32,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RXTP-A"]
[]
[]
[]
[]
["","","","","","RXTP25A2V1B","RXTP35A2V1B"]
["Dimenzije","Uređaj","","Visina","mm","605","605"]
["","","","Širina","mm","930","930"]
["","","","Dubina","mm","376","376"]
["Težina","Uređaj","","","kg","42","42"]
["Motor ventilatora","Brzina","Hlađenje","Super nisko","o/min","800","800"]
["","","Grijanje","Super nisko","o/min","400","400"]
["Compressor","Tip","","","","Hermetički zabrtvljen kompresor s klatnom","Hermetički zabrtvljen kompresor s klatnom"]
["Raspon rada","Hlađenje","Ambijent:","Min.","°CDB","-10","-10"]
["","","","Maks.","°CDB","46","46"]
["","Grijanje","Ambijent:","Min.","°CWB","-31","-31"]
["","","","Maks.","°CWB","18","18"]
["Razina tlaka zvuka","Hlađenje","","Nom.","dBA","48","48"]
["","Grijanje","","Nom.","dBA","49.0","49.0"]
["Radna tvar","Tip","","","","R-32","R-32"]
["","Punjenje","","","kg","0.97","0.97"]
["","Punjenje","","","tCO2Eq","0.66","0.66"]
["","GWP","","","","675.0","675.0"]
["Priključci cjevovoda ","Duljina cjevovoda ","Maks. ","OU - IU","m","20","20"]
["Priključci cjevovoda","Punjenje dodatne radne tvari","","","kg/m","0,02 (za duljinu cjevovoda koja premašuje 10 m)","0,02 (za duljinu cjevovoda koja premašuje 10 m)"]
["","Razlika razine","IU - OU","Maks.","m","15.0","15.0"]
["Standardna dodatna oprema","Installation manual","","","","1","1"]
["","Refrigerant charge label","","","","1","1"]
["","Multilingual fluorinated greenhouse gases labels","","","","1","1"]
["Napajanje","Faza","","","","1~","1~"]
["","Frekvencija","","","Hz","50","50"]
["","Napon","","","V","220-240","220-240"]