{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":52,"n_cols":11,"rows_kept":52,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RXZ-N"]
[]
[]
[]
[]
["","","","","","RXZ25NV1B","RXZ25NV1B9","RXZ35NV1B","RXZ35NV1B9","RXZ50NV1B","RXZ50NV1B9"]
["Razina tlaka zvuka","Grijanje","","Visoko","dBA","","","48","48","50","50"]
["","Hlađenje","","Visoko","dBA","","","48","48","49","49"]
["Standardna dodatna oprema","Radni priručnik","","","","","","1","1","1","1"]
["","Priručnik za instalaciju","","","","","","1","1","1","1"]
["Radna tvar","GWP","","","","","","675","675","675","675"]
["","Punjenje","","","kg","","","1.34","1.34","1.34","1.34"]
["","Tip","","","","","","R-32","R-32","R-32","R-32"]
["Radno područje","Hlađenje","Ambijent:","Maks.","°CDB","","","43","43","43","43"]
["","","","Min.","°CDB","","","-10","-10","-10","-10"]
["","Grijanje","Ambijent:","Maks.","°CWB","","","18","18","18","18"]
["","","","Min.","°CWB","","","-20","-20","-20","-20"]
["Priključci cjevovoda","razlika u razini","IU - OU","Maks.","m","","","8","8","8","8"]
["Dimenzije","Uređaj","","Širina","mm","","","795","795","795","795"]
["","","","Dubina","mm","","","300","300","300","300"]
["","","","Visina","mm","","","693","693","693","693"]
["Kompresor","Tip","","","","","","Hermetički zabrtvljen kompresor s klatnom_","Hermetički zabrtvljen kompresor s klatnom_","Hermetički zabrtvljen kompresor s klatnom_","Hermetički zabrtvljen kompresor s klatnom_"]
["Težina","Uređaj","","","kg","","","50","50","50","50"]
["Power supply","Faza","","","","","","1~","1~","1~","1~"]
["","Frekvencija","","","Hz","","","50","50","50","50"]
["","Napon","","","V","","","220-240","220-240","220-240","220-240"]
["Napomene","","","","","(1) - 220 V","(1) - 220 V","(1) - 220 V","(1) - 220 V","(1) - 220 V","(1) - 220 V"]
["","","","","","(2) - 230 V","(2) - 230 V","(2) - 230 V","(2) - 230 V","(2) - 230 V","(2) - 230 V"]
["","","","","","(3) - 240 V","(3) - 240 V","(3) - 240 V","(3) - 240 V","(3) - 240 V","(3) - 240 V"]
["","","","","","","","(4) - Sadrži fluorovodične stakleničke plinove","(4) - Sadrži fluorovodične stakleničke plinove","(4) - Sadrži fluorovodične stakleničke plinove","(4) - Sadrži fluorovodične stakleničke plinove"]
["Dimenzije","Uređaj","","Visina","mm","693","693"]
["","","","Širina","mm","795","795"]
["","","","Dubina","mm","300","300"]
["Težina","Uređaj","","","kg","50","50"]
["Kompresor","Tip","","","","Hermetički zabrtvljen kompresor s klatnom","Hermetički zabrtvljen kompresor s klatnom"]
["Raspon rada","Hlađenje","Ambijent:","Min.","°CDB","-10","-10"]
["","","","Maks.","°CDB","43","43"]
["","Grijanje","Ambijent:","Min.","°CWB","-20","-20"]
["","","","Maks.","°CWB","18","18"]
["Razina tlaka zvuka","Hlađenje","","Visoko","dBA","46","46"]
["","Grijanje","","Visoko","dBA","46","46"]
["Radna tvar","Tip","","","","R-32","R-32"]
["","Punjenje","","","kg","1.34","1.34"]
["","Punjenje","","","tCO2Eq","0.9","0.9"]
["","GWP","","","","675","675"]
["Priključci cjevovoda ","Duljina cjevovoda ","Maks. ","OU - IU","m","10","10"]
["Priključci cjevovoda","Razlika razine","IU - OU","Maks.","m","8","8"]
["Standardna dodatna oprema","Installation manual","","","","1","1"]
["","Operation manual","","","","1","1"]
["Napajanje","Faza","","","","1~","1~"]
["","Frekvencija","","","Hz","50","50"]
["","Napon","","","V","220-240","220-240"]