{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":37,"n_cols":7,"rows_kept":37,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RZA-D"]
[]
[]
[]
[]
["","","","","","RZA200D7Y1B","RZA250D7Y1B"]
["Dimenzije","Uređaj","","Height","mm","870","870"]
["","","","Širina","mm","1,100","1,100"]
["","","","Dubina","mm","460","460"]
["Težina","Uređaj","","","kg","117","117"]
["Kompresor","Type","","","","Hermetički zabrtvljen spiralni kompresor","Hermetički zabrtvljen spiralni kompresor"]
["Radno područje","Hlađenje","Ambijent:","Min.","°C DB","-20","-20"]
["","","","Maks.","°C DB","46","46"]
["","Grijanje","Ambijent:","Min.","°CWB","-20","-20"]
["","","","Maks.","°CWB","15","15"]
["Razina zvučne snage","Hlađenje","","","dBA","73","76"]
["","Grijanje","","","dBA","76 (1)","79 (1)"]
["Razina tlaka zvuka","Hlađenje","","Nom.","dBA","53","57"]
["","Grijanje","","Nom.","dBA","60","63"]
["Radna tvar","Tip","","","","R-32","R-32"]
["","Punjenje","","","kg","5","5"]
["","GWP","","","","675","675"]
["Priključci cjevovoda","Tekućina","","VP","mm","9.52","9.52"]
["","Plin","","VP","mm","22.2","22.2"]
["","Duljina cjevovoda","Maks.","OU - IU","m","100","100"]
["","","Sistem","Ne puni se","m","30","30"]
["","Punjenje dodatne radne tvari","","","kg/m","Pogledajte priručnik za instalaciju","Pogledajte priručnik za instalaciju"]
["Standardna dodatna oprema","Priručnik za instalaciju","","","","1","1"]
["","Opće mjere sigurnosti","","","","1","1"]
["","Vezice","","","","2","2"]
["","Skinite oznaku fluoriranih stakleničkih plinova (F-gas)","","","","1","1"]
["","Spojne cijevi","","","","6","6"]
["Power supply","Faza","","","","3~","3~"]
["","Frekvencija","","","Hz","50","50"]
["","Napon","","","V","380-415","380-415"]
["Struja - 50 Hz","Preporučeni osigurač (MFA)","","","A","20","20"]
["Napomene","","","","","(1) - U skladu s ENER serija 21","(1) - U skladu s ENER serija 21"]