{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":80,"n_cols":9,"rows_kept":80,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ATXF-C"]
[]
[]
[]
[]
["","","","","","ATXF20C5V1B","ATXF25C5V1B","ATXF42C5V1B","ATXF35C5V1B (Archived)"]
["Razina tlaka zvuka","Grijanje","","Visoko","dBA","39.0","40.0","44.0"]
["","","","Srednji","dBA","34.0","34.0","34.0"]
["","","","Tihi način rada","dBA","21.0","21.0","22.0"]
["","","","Nizak","dBA","28.0","28.0","28.0"]
["","Hlađenje","","Srednji","dBA","33.0","33.0","36.0"]
["","","","Tihi način rada","dBA","20.0","20.0","22.0"]
["","","","Nizak","dBA","25.0","26.0","30.0"]
["","","","Visoko","dBA","39.0","40.0","45.0"]
["Standardna dodatna oprema","Priručnik za instalaciju","","","","1","1","1"]
["","Radni priručnik","","","","1","1","1"]
["","Baterije","","","","1","1","1"]
["","Infracrveno daljinsko upravljanje","","","","1","1","1"]
["","AAA suhe baterije","","","","2","2","2"]
["","Držač daljinskog upravljača","","","","1","1","1"]
["","Montažna ploča","","","","1","1","1"]
["","Učvrsni vijak unutarnje jedinice","","","","2","2","2"]
["Upravljački sustavi","Žično daljinsko upravljanje","","","","BRC073A1","BRC073A1","BRC073A1"]
["","Infrared remote control","","","","ARC470A1","ARC470A1","ARC470A1"]
["Priključci cjevovoda","Tekućina","","VP","mm","6.35","6.35","6.35"]
["","Plin","","VP","mm","9.50","9.50","9.50"]
["","Odvod vode","","","","18","18","18"]
["Ulazna struja","Hlađenje","","Nom.","kW","0.023","0.023","0.040"]
["","Grijanje","","Nom.","kW","0.023","0.023","0.040"]
["Razina zvučne snage","Hlađenje","","","dBA","53.0","54.0","59.0"]
["","Grijanje","","","dBA","55.0","55.0","59.0"]
["Dimenzije","Uređaj","","Širina","mm","770","770","770"]
["","","","Dubina","mm","225","225","225"]
["","","","Height","mm","286","286","286"]
["Kućište","Boja","","","","Bijelo","Bijelo","Bijelo"]
["Težina","Uređaj","","","kg","8.00","8.00","9.00"]
["Power supply","Phase","","","","1~","1~","1~"]
["","Frekvencija","","","Hz","50","50","50"]
["","Napon","","","V","220-440","220-440","220-440"]
["Ulazna struja","Hlađenje","","Nom.","kW","","","","0.029"]
["","Grijanje","","Nom.","kW","","","","0.029"]
["Kućište","Boja","","","","","","","Bijelo"]
["Dimenzije","Uređaj","","Visina","mm","","","","286"]
["","","","Širina","mm","","","","770"]
["","","","Dubina","mm","","","","225"]
["Težina","Uređaj","","","kg","","","","8.5"]
["Ventilator","Količina zraka","Hlađenje","Visoko","m³/min","","","","11.8"]
["","Protok zraka","Hlađenje","Srednji","m³/min","","","","8"]
["","","","Nizak","m³/min","","","","6.4"]
["","","","Tihi način rada","m³/min","","","","4.4"]
["","","Grijanje","Visoko","m³/min","","","","11.9"]
["","Protok zraka","Grijanje","Srednji","m³/min","","","","8.6"]
["","","Grijanje","Nizak","m³/min","","","","6.5"]
["","","","Tihi način rada","m³/min","","","","5.3"]
["Zvučna snaga","Hlađenje","","","dBA","","","","54"]
["","Grijanje","","","dBA","","","","56"]
["Razina tlaka zvuka","Hlađenje","","Visoko","dBA","","","","43"]
["Razina zvučnog tlaka","Hlađenje","","Srednji","dBA","","","","34"]
["Razina tlaka zvuka","Hlađenje","","Nizak","dBA","","","","27"]
["","","","Tihi način rada","dBA","","","","20"]
["","Grijanje","","Visoko","dBA","","","","40"]
["Razina zvučnog tlaka","Grijanje","","Srednji","dBA","","","","35"]
["Razina tlaka zvuka","Grijanje","","Nizak","dBA","","","","29"]
["","","","Tihi način rada","dBA","","","","21"]
["Priključci cjevovoda","Tekućina","","VP","mm","","","","6.35"]
["","Plin","","VP","mm","","","","9.5"]
["","Odvod vode","","","","","","","18"]
["Upravljački sustavi","Infracrveno daljinsko upravljanje","","","","","","","ARC470A1"]
["","Žično daljinsko upravljanje","","","","","","","BRC073A1"]
["Standardna dodatna oprema","Installation manual","","","","","","","1"]
["","AAA dry-cell batteries","","","","","","","2"]
["","Operation manual","","","","","","","1"]
["","Batteries","","","","","","","1"]
["","Indoor unit fixing screws","","","","","","","2"]
["","Infrared remote control","","","","","","","1"]
["","Mounting plate","","","","","","","1"]
["","Remote control holder","","","","","","","1"]
["Napajanje","Faza","","","","","","","1~"]
["","Frekvencija","","","Hz","","","","50"]
["","Napon","","","V","","","","220-440"]